[04:28:51] setup | Starting firmware: v2.3.6\n[04:28:52] ConfigHelper | LittleFS mounted\n[04:28:52] ConfigHelper | load config\n[04:28:52] ConfigHelper | config open: Ok\n[04:28:52] setup | Config loaded\n[04:28:52] setup | Reboot reason: 3\n[04:28:52] setup | Coordinator mode: LAN\n[04:28:52] setup | Device type: SLZB-06P10\n[04:28:52] setup | Radio mode: \"ZB COORD\" Radio FW version: 20240716 Radio FW CH: PROD\n[04:28:52] Network | init\n[04:28:52] L_Y,L_B | status: 1\n[04:28:54] Network | EVENT_ETH_START\n[04:28:54] Network | EVENT_ETH_CONNECTED\n[04:28:54] Network | [MDNS] Started\n[04:28:54] Network | EVENT_ETH_GOT_IP\n[04:28:54] Network | ETH MAC: AA:BB:CC:DD:EE:FF IPv4: 192.168.0.11 GW: 192.168.0.1 Speed: 100Mbps DNS1: 192.168.0.1 DNS2: 0.0.0.0\n[04:28:54] Network | fireNetworkUp\n[04:28:54] taskZB | Waiting for zbChk\n[04:28:54] Web | Webserver started